Isuzu 4475 Wrecker Truck Technical Agreement Summary
Chassis Specifications
	Specification
	Details

	Model
	QL1100A8MAY 4*2

	Engine Model
	Isuzu 4HK1-TC51

	Engine Power
	190 horsepower

	Fuel Type
	Diesel

	Emission Standard
	Euro V

	Transmission
	6-speed Isuzu MLD gearbox

	Brakes
	ABS, air-operated

	Suspension
	Front axle 4 tons, rear axle 7 tons

	Tires
	6 + 1 (235/75R17.5)

	Dimensions
	Total length 7930 mm, width 2170 mm, height 2350 mm

	Wheelbase
	4475 mm

	Gross Weight
	10,000 kg

	Empty Weight
	3210 kg


Body Specifications
	Specification
	Details

	Platform Design
	Half-floor

	Carrying Capacity
	5 tons

	Platform Dimensions (External)
	6200mm x 2400mm

	Platform Dimensions (Internal)
	6000mm x 2300mm

	Platform Tilt Angle
	8°

	Working Stroke
	2700 mm

	Platform Height
	1290 mm

	Winch Rated Pulling Force
	50 kN, wire rope diameter φ11mm, length 25m


Hydraulic and Other Features
	Specification
	Details

	Hydraulic Stabilizers
	Can be operated independently or together

	Operation System
	Dual-side operation

	Additional Equipment
	4 straps, auxiliary cart, standard tools, stainless steel hand-washing box, chain hook, national standard warning lights


Vehicle Overall Parameters
	Specification
	Details

	Model
	CLW5100TQZQ5

	Dimensions
	8100mm x 2400mm x 2350mm

	Curb Weight
	5660 kg

	Spring Leaves
	8/10+6

	Maximum Speed
	110 km/h

	Seating Capacity
	3 people






